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	To
	:
	

	Attention
	:
	

	Ref
	:
	
	Voyage
	:
	
	C/P Date
	:
	


For the purposes of planning and carrying out a risk assessment prior to the intended STS operation, a reply to the following questionnaire is requested. Failure to reply may result in delays to the intended operation.

IMPORTANT NOTE:

Company has a policy that all STS transfers MUST be conducted per the ICS / OCIMF Ship-to-Ship Transfer Guide.  It should be noted that company strongly discourages STS berthing operations during the hours of darkness due to safety reasons, however if situation demands then this to be discussed with the Marine Manager and Risk assessment conducted. 

The information provided from the Masters, calling upon the Agents for the specifics, below should be forwarded to Marine department for their review. 

Company reserves the right to request our principles to refuse an STS operation if they deem it unsafe as a result of:

a.
Unsuitable lightering vessel nominated for the operation.

b.
Inadequate facilities, permissions or equipment to conduct a safe STS transfer.

c.
Inadequate or incorrect procedures intended for the operation

	AA. 
STS VESSEL DETAILS:

	
	Parameter
	Information

	1.1 
	Name of Vessel
	

	1.2 
	IMO/Lloyds number
	

	1.3 
	Flag/Class/Built
	

	1.4 
	Current Owner/Operator details
	

	1.5 
	Date of last SIRE inspection:

Not older than 6 months
	

	1.6 
	Ships manifold in compliance with OCIMF?
	

	1.7 
	Ships lifting equipment in accordance with OCIMF?
	

	BB.
STS TRANSFER COMPANY / EQUIPMENT DETAILS:

	
	Parameter / Information
	Information

	2.1
	Name of Company appointed to conduct STS operation?
	

	2.2
	STS position – Place or Latitude / Longitude?
	

	2.3
	Intended STS berthing operation underway / anchor?
	

	2.4
	Intended cargo transfer conducted at underway / anchor?
	

	2.5
	Number / Type / Size / Position of primary fenders?
	

	2.6
	Number / Type / Size / Position of secondary fenders?
	

	2.7
	Number / Length / Size of cargo hoses?
	

	CC.
OPERATIONS DETAILS:

	
	Parameter / Information
	Information

	3.1
	Bridge Team, including Master’s STS experience.

Has Bridge Team referred to STS Manoeuvring & Mooring guidance, in addition to ICS STS transfer guide?

Does the bridge team fully understands the Hydrodynamic interaction between the two loaded vessels when approaching each other during STS operations
	

	3.2
	Confirm the Vessel’s carried out STS Mooring drill to the satisfaction of Master.
	

	3.3
	Are the operations planned for Daylight?

If the operations are not planned for daylight, kindly attached a completed risk assessment for Office concurrence for same. 
	

	3.4
	Weather Condition ( Wind dir / force, Sea & Swell ) 

Any Adverse Weather warnings
	

	3.4
	The Draught / Trim of manoeuvring vessel? 

It is preferred to have the manoeuvring vessel to have a trim of 1m or more. If the trim is less than 1.0 mtrs, what risk control measures are being taken implemented in order to deal with the reduced manoeuvrability of the  manoeuvring vessel
	

	3.5
	Positions of the primary & secondary fenders are as per guidance given as per section 9.1.1 of ICS STS transfer guide. ( Guidance attached  )
	

	3.6
	In case of underway STS operations, Confirm that the operations would be conducted at speed of 5.0 kts or less.
	

	3.7
	Are Tug/s being used for the operations?

It is preferred to use tug/s for STS operations. Kindly attach a completed risk assessment in case tugs are not available. 
	

	3.8
	Panama flagged vessels: has the notification to flag done at least 48 hours prior planned STS operation on E-Segumar Platform at the link?- https://certificates.amp.gob.pa/certificates              
	

	3.9
	Panama Flagged Vessels: Has the acknowledgement of receipt from Flag receipt for the Notification of STS planned operation.
	

	3.10
	a) Panama Flagged Vessels: If the estimated time of arrival of an oil tanker at the location or area for the STS transfer operation changes by more than six hours or in the event that the STS operation is cancelled due to any issue, the Master, Owner, or Designated Person Ashore (DPA) must immediately inform the Administration via the following email address : stspma@amp.gob.pa

	

	3.11
	Panama Flagged Vessels: The STS transfer notification shall include the following information:

I) Name, flag, call sign, IMO Number and estimated time of arrival of the oil tankers involved in the STS transfer operation.

II) Date, time and geographical position of the commencement of the planned STS transfer operation.

III) Mode in which the STS transfer operation will be carried out: at anchor or underway.
IV) Type of oil and its quantity.
V) Expected duration of the STS transfer operation.

VI) Identification and contact information (email, telephone number) of the Designated Person Ashore (DPA) of each oil tanker involved in the STS operation.

VII) Confirmation that the oil tanker has on board an STS operations Plan complying the requirements of regulation 41, Annex I, MARPOL Convention


	

	3.12
	All the Panamanian flagged oil tankers must maintain valid and updated Continuous Synopsis Record (CSR) and Conformance Test Report (CTR) on board at the time of notifying the STS operations. Failure to comply with the aforementioned will result denying the authorization for STS operations until compliance is demonstrated.
	



