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	At sea ship to ship transfer
(Between ship operator / charterer and organiser)

	Ship Operator:


	Ship Charterer:


	STS Organizer:



	Ship’s Name
	:
	
	Company
	: 
	

	Call Sign / INMARSAT No
	:
	
	Proposed Date of Transfer
	: 
	

	IMO Number
	:
	
	Proposed Location
	:
	


	Discharging / Receiving Ship (Delete as appropriate)
	Ship Operator’s Confirmation
	Remarks

	1
	Current vessel particulars questionnaire (VPQ) data has been exchanged
	
	

	2
	Stage the anticipated maximum berthing displacement of the ship
	
	

	3
	Stage the anticipated arrival draughts and freeboard
	
	

	4
	If the berthing operation is to be conducted underway, confirm that the ship can maintain about five knots for a minimum of two hours
	
	

	5
	The ship is able to conduct operation in accordance with the latest edition of the Ship to Ship Transfer Guide
	
	

	6
	Sufficient manpower will be provided to ensure the safe conduct of operation while minimizing the potential for fatigue
	
	

	7
	Key vessel personal can communicate in English, If not, stage working language used
	
	Working language: English

	8
	The ship’s manifold arrangement and lifting gear is in accordance with OCIMF or SIGTTO recommendations for the ship type/size
	
	

	9
	Stage the maximum and minimum expected height of the cargo manifold from the waterline during the transfer
	
	Max:                         m

Min :                         m

	10
	The SWL and outreach of the ship’s lifting equipment is sufficient for the intended operation
	
	SWL:                        Tons

Outreach:                 m

	11
	Where applicable, a copy of the STS operations plan has been exchanged
	
	

	12
	If not included within the STS operations plan, a general arrangement plan or other similar mooring diagram has been exchanged
	
	

	13
	The location and number of enclosed fairleads and mooring bitts fitted on the ship is in accordance with Mooring Equipment Guidelines (reference 6)
	
	

	14
	The ship is able to deploy all lines in winch drums
	
	

	15
	Messenger lines of suitable strength will be available at each mooring location
	
	

	16
	MSDS information has been exchanged for the cargo being transferred and, where applicable, the previous cargo of the receiving ship
	
	

	17
	Both side of the ship are clear of any overhanging projections, including bridge wings
	
	

	18
	Sufficient accommodation is available on board for STS personal
	
	

	Additional for Oil Transfer:

	19
	Confirm the vessel is equipment to conduct vapour balancing
	
	

	Additional for LPG Transfers:

	20
	State the arrangement of liquid and vapour manifold connections
	
	

	Additional for LNG Transfers:

	21
	STS Transfer Compatibility Questionnaire data has been exchanged 
	
	

	For discharging / receiving ship (Delete as appropriate)

	Name
	: 
	

	Rank or Position in Company
	: 
	

	Signature:
	
	Date:
	



