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	Discharging Ship’s Name
	:
	

	Receiving Ship’s Name
	:
	

	Name of Designated POAC
	:
	

	Name of STS Superintendent if Different from POAC
	:
	

	Date and Location of Transfer
	:
	


	Items
	Checked
	Remarks

	1
	A copy of the completed checklist 1 has been received
	
	

	2
	A copy of the JPO that encompasses the entire transfer operation has been received
	
	

	3
	Personal will comply with the hours of work and rest requirements of IMO and national regulations, as appropriate
	
	

	4
	Radio communications, including back-up system, have been agreed and tested and clocks have been synchronized between the ships
	
	

	5
	The language of operations has been agreed
	
	Working language: English

	6
	The rendezvous position of the transfer area has been agreed
	
	

	7
	Information on ship handling characteristics has been exchanged, including details of any critical main engine revolutions and corresponding speed
	
	Ship Particulars exchanged with all details

	8
	Approach, manoeuvring and mooring plans are understood and confirmed
	
	

	9
	Mooring procedures have been agreed, including fender positions and number /type of ropes to be provided by each ship
	
	

	10
	The system and method of electrical insulation between ships has been agreed
	
	

	11
	The ships are upright and at a suitable trim, without any overhanging projections
	
	

	12
	Manoeuvring, mooring and navigational equipment has been tested and found in good order 
	
	

	13
	Cargo transfer system safety devices, including IG and emergency shutdown (ESD) systems, where applicable, have been proven operational not more than 48-hours prior to the operation
	
	

	14
	The Ship’s boilers and tubes have been cleared of soot and it is understood that during STS operations, tubes must not be blown
	
	

	15
	Engineers have been briefed on engine speed (and speed adjustment) requirements
	
	

	16
	Weather forecasts have been reviewed for the transfer area and arrangements have been made for their continued receipt throughout the operation
	
	

	17
	The hose lifting equipment is suitable and ready for use
	
	

	18
	The cargo transfer hoses/arms have been tested and certified and they are in apparent good condition
	
	Cargo Hoses last Press & Continuity Tested on:



	19
	The fenders and associated equipment are visually in apparent good order
	
	Fender last Pr Tested on:



	20
	The crew have been briefed on the mooring procedure
	
	

	21
	The contingency plan is agreed, and an appropriate emergency drill has been conducted
	
	

	22
	Local authorities have been advised about the operation
	
	

	23
	A navigational warning has been broadcast
	
	

	24
	Monitoring is in place for accommodation, void spaces, pumproom, compressor and motor rooms, as applicable, to detect possible flammable atmospheres
	
	

	25
	The other ship has been advised the checklist 2 is satisfactorily completed
	
	Local Time:             

	Additional for LNG and LPG transfers:

	26
	Cargo lines have been cooled 
	
	

	FOR DISCHARGING / RECEIVING SHIP (Delete as appropriate)

	Name
	: 
	

	Rank or Position in Company
	: 
	

	Signature
	:
	Date
	:



