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	Discharging ship’s name:
	Name of STS Organiser /
 Superintendent:

	Company
	: 
	
	

	Call Sign / INMARSAT No
	:
	
	Date of Transfer:
	
	

	IMO Number
	:
	
	Location:
	
	

	Receiving ship’s name
	:
	
	
	
	

	Company
	: 
	
	
	
	

	Call Sign / INMARSAT No
	:
	
	
	
	

	IMO Number
	:
	
	
	
	


	
	Repetitive 

Check 1
	Repetitive Check 2
	Repetitive Check 3

	1
	Present weather and sea conditions are within the agreed limits
	
	
	

	2
	Personal engaged in the cargo transfer operation are wearing appropriate PPE
	
	
	

	3
	Cargo hose strings, manifold connections and cargo system are free of any leakage
	
	
	

	4
	Cargo hose are properly supported, considering changing freeboards and any movement between the vessels
	
	
	

	5
	All cargo monitoring system, including level gauges, high level alarms, pressure gauges and alarms, are functioning correctly
	
	
	

	6
	The cargo transfer operation is continuing under closed conditions
	
	
	

	7
	The sea surface around the vessel is periodically visually checked for any signs of pollution
	
	
	

	8
	All identified spaces are being routinely monitored for any build-up of flammable and/or toxic vapour 
	
	
	

	9
	All mooring line are correctly tensioned and managed / monitored during cargo transfer / double banking
	
	
	

	10
	Where rigged in accordance with local requirements, emergency towing-off pennants are adjusted throughout the cargo transfer operation
	
	
	

	11
	On completion of cargo transfer to or from a tank, the tank is secured
	
	
	

	12
	Levels in all cargo and ballast tanks, including those not being worked, are routinely monitored.
	
	
	

	Checked By:
	
	
	

	Date & Time:
	
	
	



