



SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	COMMENCEMENT OF LOADING AT TERMINAL

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 1.119


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	Commencement of loading before the ship becomes ready.
	Moderate  cost or damage
	Start loading when all necessary terminal & tanker valves in the loading system are open & the ship has signified readiness.
	1
	3
	3

	2
	Wrong setting of valves.
	Moderate  cost or damage
	Whenever possible, the initial flow should be by gravity, at slow rate and to a single tank.
	1
	3
	3

	3
	Designation of wrong tank.
	Moderate  cost or damage
	Start shore pumps after system has been checked & the ship advises that cargo is being received in the correct tank(s).
	1
	3
	3

	4
	Manifold leaks.
	Moderate  cost or damage
	After starting the pumps, check the ship & shore connections for tightness until the agreed flow rate or pressure is reached.
	1
	3
	3

	5
	Leakage in the pump-room when loading by pump-room drop lines.
	Moderate  cost or damage
	Avoid. Whenever possible, load cargo through drop lines within the cargo tank area, with all pump room valves closed.
	1
	3
	3

	6
	Wrong grade of cargo is being loaded.
	Moderate  cost or damage
	Take cargo sample a.s.a.p. after commencement of loading & before opening up subsequent tanks for loading.
	1
	3
	3

	7
	Static electricity dangers during sampling non-inerted tanks loading static accumulator cargoes.
	Moderate  cost or damage
	Follow safe sampling practices.
	1
	3
	3

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	
	
	
	
	
	
	

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	EMERGENCY SITUATION
	REFER TO COMPANY’S EMERGENCY PROCEDURES MANUAL.


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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