

SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	MOORING OPERATION – DEPLOYMENT OF SPRING LINES

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 1.26


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	During mooring operation, the vessel was slowly manoeuvring alongside the jetty with two mooring wires deployed forward from the aft most winch and two wires deployed aft from the forward most winch.

As the vessel was coming alongside there was a difference in the tension on the two wires and it was allowed to build up so that only one wire rope was bearing the main load.

With about 1 meter to go astern, the weight came on the single fwd wire and before it could be slacked, the wire partied.

(The tension was allowed to become too excessive on the single mooring wire, as the vessel fell back resulting in the wire parting).
	· Moderate  cost or damage

· Injury of personnel


	· Safety precautions during mooring operations as described in company’s safety management system.

· Inspection of mooring wires before every mooring operation.

· Training / familiarization

· Personal Protective Equipment (PPE)


	4
	3
	12

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	1
	A. When two wires or ropes are deployed to the same direction, these should be adjusted prior to heaving up as the vessel approaches the jetty in order to balance the load equally and prevent breaking or any other incident.
	Deck officer in charge
	During operation
	1
	3
	3

	
	B. Consideration to be made to allow for the wires to be supplied with an eye each and to facilitate turning at mid life.
	Operations Manager
	During operation
	
	
	

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	DECK EQUIPMENT FAILURE, SERIOUS INJURY
	REFER TO COMPANY’S SHIP EMERGENCIES AND COMPANY’S CONTIGENCY PLANS.


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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