

















SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	USE OF WORK EQUIPMENT

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 3.19  


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	· Electrocution
· Mechanical Injury / Burns
· Eye Injuries

· Operating Machinery

· Noise
	Serious injury
	Company’s established procedures and safety practices within IMS 
· Chapter 20 “Use of Work Equipment” of “The Code of Safe Working Practices for Merchant Seamen” should always be consulted

· Knowledge of proper operation of tools & equipment to be ascertained by responsible officer.
· Relative humidity of the atmosphere must be monitored.              

· Weather and sea condition (raining, pitching, and rolling) always must be taken into account.

· Operator to be fully trained in the use of tools/equipment.

· Knowledge of emergency stops is required by all personnel.                                          

· Correct PPE must be worn.

· Correct eye protection must be worn where required.

· Correct hearing protection to be worn.                       

· Check for proper operation of the tools and equipment before use.

· Rest hours of all involved personnel are always taken into account.
	3
	3
	9

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	1
	A. Only experienced and qualified personnel to be involved in the use of tools & equipment.
	C/E
	Before & During Task
	3
	2
	6

	
	B. Clear/strict instructions should be given to all personnel involved in the painting works so that if any of the existing control measures are not in line with Company’s requirements, the work should be suspended and the Chief Engineer should be immediately informed.
	C/E
	Before & During Task
	
	
	

	
	C. Clear/strict instructions should be given to all personnel involved in painting works so that if any of the existing control measures are not adequate /enough with the specific task given, they should consult the Chief Engineer before commencing the work.
	C/E
	Before Task
	
	
	

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	SERIOUS INJURY
	REFER TO COMPANY’S CONTIGENCY PLANS.


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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